Loading instructions for the CPxx5 Operating System.


1. With the power OFF, insert the first disk into the disk drive on the CP model to be loaded.

2. Turn the power ON. The CP will read the disk and after a few seconds begin loading the data. 

    First, two small circles will appear at the top of the display, then a row of circles across which turn 
    from white to black as the data is loading.  When the disk is finished loading, the display will show "Complete". 

3. Turn the power OFF and insert the next disk.

4. Follow steps 1-3 until you have successfully loaded all of the disks for the CP model you are loading.
    

If for any reason the row of circles does not appear, simply try that disk again.  Power off and back on.

Note: While there is no specific loading order for the disks we recommend that you load them in the order they are 
         organized in the list below.

Also, there is a RESET button located in the Conductor area.  Hold this while turning on the power after completing
the entire loading process - - wait until you hear a "click", then release.
This is a hard reset for the machine.  Soft reset can be found in the System pages.
===================================================================================
File List:

CP5H_000.SYS 	TG O/S for CP205/175/155
CP5HC000.SYS 	TG O/S for CP185 ONLY (replaces H_000)
CP5H_100.SYS 	initial user data
CP5HT180.SYS 	tone parameter
CP5H_200.SYS 	registration data
CP5H_300.SYS 	demo data
CP5H_400.SYS 	style data 1
CP5H_500.SYS 	style data 2
CP5H_600.SYS 	style data 3
CP5H_700.SYS 	style data 4
CP5L_000.SYS 	LCD O/S
CP5L_100.SYS 	LCD data 1
CP5L_200.SYS 	LCD data 2
CP5L_300.SYS 	LCD data 3
CP5L_400.SYS 	LCD data 4
CP5L_500.SYS 	LCD data 5
CP5L_600.SYS 	Piano Music data
CP5C_E00.SYS 	CD O/S for CP205/175
====================================================================================
To see the current OS version:

Power up the CPxx5, wait for Main Screen
Push SYSTEM button
Select PAGE 2 at the bottom of screen
Select Software Version on right side of screen
