KAWAI USB-MIDI
DEVICE DRIVER INSTALL

This is how to install KAWAI USB-MIDI driver.
for WindowsVista
for WindowsXP
for Windows2000
for Windows98SE
仸After driver installation, please select
丂[KAWAI USB MIDI IN]丄or [KAWAI USB MIDI OUT] in your application software.
仸Not supported under 64-bit WindowsXP or Vista

for WindowsVista

1.Do not connect the USB cable yet.
2.Installing the Driver files.
丂丂丂丂仠Open the extracted folder named 'KAWAI-USB-MIDI'.
丂丂
丂丂丂丂仠Right-click [setup] file in [KAWAI-USB-MIDI] folder and click [Properties].
丂丂
丂丂丂丂仠Click [Compatibility] tab when [setup Propaties] dialog is displayed.
丂丂
丂丂丂丂仠Click [Run this program in compatibility mode for.].
丂丂丂丂丂Verify the selected list named 'Windows XP (Service Pack 2)' and click [OK].
丂丂丂丂丂仸If not, select 'Windows XP (Service Pack 2)' by click.
丂丂
丂丂丂丂仠Right-click [setup] file in [KAWAI-USB-MIDI] folder and click [Run as administrator].
丂丂丂丂丂仸If computer prompts you for an administrator password or for a confirmation,
丂丂丂丂丂丂type the password, or click [Continue].
丂丂
丂丂丂丂仠Click [Allow] when [User Account Control] dialog is displayed.
丂丂丂丂丂[SETUP MIDI DRIVER]-[Install USB Driver] will be displayed.
丂丂
丂丂丂丂仠Click [Yes]. Click [Install this driver software anyway] when [Windows Security] dialog is displayed.
丂丂
丂丂丂丂仠After a short time, [SETUP MIDI DRIVER]-[SETUP Completed] will be displayed.
丂丂丂丂丂Click [OK].
丂丂
3.Turn the power on for the digital piano and connect to computer with a USB cable.
丂丂丂丂仠When you connect to computer with a USB cable, the following message appears.
丂丂丂丂 It is necessary to update the driver.
丂丂
4.Launching the Device Manager.
丂丂丂丂仠Click the start button at the lower-left corner of the desktop. Click [Control Panel] afer menu is displayed.
丂丂
丂丂丂丂仠Click [Classic View] when [Control Panel] window is displayed.
丂丂
丂丂丂丂仠Double-click [Device Manager].
丂丂丂丂丂Click [Continue] when [User Account Control] dialog is displayed.
丂
丂丂丂丂仠[Device Manager] window will be displayed.
丂丂丂丂丂[USB-MIDI] will be displayed under [Sound, video and game controllers].
丂丂
5.Updating driver software.
丂丂丂丂仠Right-click [USB-MIDI], and click [Update Driver Software...] when menu is displayed.
丂丂
丂丂丂丂仠Click [Browse my computer for driver software].
丂丂
丂丂丂丂仠Click [Let me pick from a list of device drivers on my computer].
丂丂
丂丂丂丂仠Click [KAWAI USB MIDI].
丂丂
丂丂丂丂仠Click [Next] when [KAWAI USB MIDI] is displayed inverted.
丂丂
丂丂丂丂仠Click [Close] to exit Devie Driver install.
丂丂丂丂丂
丂丂
丂丂丂丂仠Click [YES] to restart your computer.
丂丂

for WindowsXP

In the case that the standard USB driver(USB audio device) does not work by anything cause, please install the KAWAI USB-MIDI driver.
*note: Usually,there is not the necessity.
1.Do not connect the USB cable yet.
2.Double click [setup.exe] in KAWAI-USB-MIDI folder.
仠Click "Yes" when the dialog below is displayed.
丂丂
仠If the dialog below is displayed, click "ContinueAnyway" to continue the installation.
丂丂
仠Click "OK" to finish when the dialog below is displayed.
丂丂
3.Turn the power on for the digital piano and connect to the computer with the USB cable.
仠Because the standard USB driver (USB audio device) have priority in installation, please exchange the driver with the follow procedure to complete the installation of the KAWAI USB-MIDI driver.
4.Start the Device Manager.
仠Click "Start" and Select "Control Panel" in the menu.
丂丂
仠Click "Switch to Classic View" when the "Pick a category"menu is displayed.
丂丂
仠Click the icon of "System".
丂丂
仠The dialog of "System Properties" is displayed. Click "Hardware" tub and click "Device Manager".
丂丂
仠"Device Manager" is started. Dubble click "Sound, video and game controllers".
丂丂
5.Exchange the driver.
仠Right click "USB Audio Device" and select "Update Driver..."
丂丂
仠"Hardware Update Wizard" is started. If the following is appeared, select "No,not this time" and click "Next".
丂丂
仠Select "Install from a list or specific location(Advanced)" and click "Next".
丂丂
仠Select "Don't search. I will choose the driver to install." and click "Next".
丂丂
仠Select "KAWAI USB MIDI" and click "Next".
丂丂
仠Click 乬Continue Anyway乭 to continue the installation if the following is appeared.
丂丂
仠Click乬Complete乭to finish the wizard. Installation of the device driver is completed.
丂丂
仠Restart the computer.
丂丂

for Windows2000

侾丏Do not connect the USB cable yet.
俀丏Double click [setup.exe] in KAWAI-USB-MIDI folder.
丂丂丂丂仠Click 乬Yes乭 when the dialog below is displayed.
丂丂
丂丂丂丂仠The dialog below is displayed. Click 乬Yes乭 to continue the installation.
丂丂
丂丂丂丂仠Click 乬OK乭 to finish when the dialog below is displayed.
丂丂
俁丏Turn the power on for the digital piano and connect to the computer with the USB cable.
丂丂丂丂仠乬Found New Hardware 乭 below is displayed.
丂丂丂丂
丂丂丂丂丂 Click 乬Yes乭 to continue the installation.
丂丂
丂丂丂丂仠Click 乬Complete乭 to finish the wizard. Installation of the device driver is completed.
丂丂
丂丂丂丂仠Restart the computer.
丂丂

for Windows98SE

1.Do not connect the USB cable yet.
2.Double click [setup.exe] in [KAWAI-USB-MIDI] folder.
丂丂丂丂仠Click [YES] when the dialog below is displayed.
丂丂
丂丂丂丂仠Click [OK] to finish when the dialog below is displayed.
丂丂
Turn the power on for the digital piano and connect to the computer with the USB cable.
丂丂丂丂仠When [new hardware addition wizard] is displayed, click [Next] to finish the wizard.
丂丂丂丂仠Installation of the device driver is completed.